$OpenBSD: patch-hccontrol_hccontrol_8,v 1.1 2005/07/17 18:20:29 grange Exp $
--- hccontrol/hccontrol.8.orig	Sun Jul 17 22:08:51 2005
+++ hccontrol/hccontrol.8	Sun Jul 17 22:12:56 2005
@@ -30,20 +30,17 @@
 .Os
 .Sh NAME
 .Nm hccontrol
-.Nd HCI configuration utility
+.Nd Bluetooth HCI control utility
 .Sh SYNOPSIS
 .Nm
 .Op Fl hN
-.Fl n Ar HCI_node_name
+.Fl n Ar interface
 .Ar command
 .Op Ar parameters ...
 .Sh DESCRIPTION
 The
 .Nm
-utility connects to the specified Netgraph node of type
-.Dv HCI
-and attempts to send specified command to the HCI Netgraph node or to the
-associated Bluetooth device.
+utility sends specified command to the Bluetooth network interface.
 The
 .Nm
 utility will print results to the standard output and error messages to
@@ -58,8 +55,8 @@ Show Bluetooth addresses as numbers.
 Normally
 .Nm
 attempts to resolve Bluetooth addresses, and display them symbolically.
-.It Fl n Ar HCI_node_name
-Connect to the specified HCI Netgraph node.
+.It Fl n Ar interface
+Use specified network interface, e.g. ubt0.
 .It Ar command
 One of the supported commands (see below).
 Special command
@@ -81,7 +78,7 @@ The currently supported HCI commands in
 .Nm
 are:
 .Pp
-.Bl -tag -offset indent -compact
+.Bl -tag -width indent -compact
 .It Cm Inquiry
 .It Cm Create_Connection
 .It Cm Disconnect
@@ -148,7 +145,7 @@ The currently supported node commands in
 .Nm
 are:
 .Pp
-.Bl -tag -offset indent -compact
+.Bl -tag -width indent -compact
 .It Cm Read_Node_State
 .It Cm Initialize
 .It Cm Read_Debug_Level
@@ -172,9 +169,7 @@ are:
 .Ex -std
 .Sh SEE ALSO
 .Xr bluetooth 3 ,
-.Xr netgraph 3 ,
-.Xr netgraph 4 ,
-.Xr ng_hci 4 ,
+.Xr ubt 4 ,
 .Xr hcseriald 8
 .Sh AUTHORS
 .An Maksim Yevmenkin Aq m_evmenkin@yahoo.com
