$OpenBSD: patch-doc_saned_man,v 1.4 2008/02/13 13:23:58 ajacoutot Exp $
--- doc/saned.man.orig	Sat Nov 26 06:31:26 2005
+++ doc/saned.man	Tue Feb 12 11:40:39 2008
@@ -92,7 +92,7 @@ support IPv6, check the documentation for your inetd d
 The configuration line normally looks like this:
 .PP
 .RS
-sane-port stream tcp nowait saned.saned @SBINDIR@/saned saned
+sane-port stream tcp nowait _saned._saned @SBINDIR@/saned saned
 .RE
 .PP
 However, if your system uses
@@ -105,16 +105,16 @@ and use a line of the following form in
 instead:
 .PP
 .RS
-sane-port stream tcp nowait saned.saned /usr/sbin/tcpd @SBINDIR@/saned
+sane-port stream tcp nowait _saned._saned /usr/libexec/tcpd @SBINDIR@/saned
 .RE
 .PP
 Note that both examples assume that there is a
-.B saned
+.B _saned
 group and a
-.B saned
+.B _saned
 user.  If you follow this example, please make sure that the 
 access permissions on the special device are set such that
-.B saned
+.B _saned
 can access the scanner (the program generally needs read and
 write access to scanner devices).
 .PP
@@ -133,8 +133,8 @@ service sane-port
    port        = 6566
    socket_type = stream
    wait        = no
-   user        = saned
-   group       = saned
+   user        = _saned
+   group       = _saned
    server      = @SBINDIR@/saned
 }
 .fi
