(export (version D)
  (design
    (source /home/ashton/repo/kicad-library/template/raspberrypi-gpio-40pin/raspberrypi-gpio-40pin.sch)
    (date "Mon 04 Sep 2017 07:54:14 AM CDT")
    (tool "Eeschema (2017-02-21 revision 35a8d78)-master")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date "15 nov 2012")
        (source raspberrypi-gpio-40pin.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P1)
      (value Conn_02x20_Odd_Even)
      (libsource (lib conn) (part Conn_02x20_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AD464A)))
  (libparts
    (libpart (lib conn) (part Conn_02x20_Odd_Even)
      (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)")
      (docs ~)
      (footprints
        (fp Connector*:*2x??x*mm*)
        (fp Connector*:*2x???Pitch*)
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x20_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))
        (pin (num 33) (name Pin_33) (type passive))
        (pin (num 34) (name Pin_34) (type passive))
        (pin (num 35) (name Pin_35) (type passive))
        (pin (num 36) (name Pin_36) (type passive))
        (pin (num 37) (name Pin_37) (type passive))
        (pin (num 38) (name Pin_38) (type passive))
        (pin (num 39) (name Pin_39) (type passive))
        (pin (num 40) (name Pin_40) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /home/ashton/repo/kicad-library/library/conn.lib)))
  (nets
    (net (code 1) (name "/GPIO4(GCLK)")
      (node (ref P1) (pin 7)))
    (net (code 2) (name "/GPIO3(SCL1)")
      (node (ref P1) (pin 5)))
    (net (code 3) (name +5V)
      (node (ref P1) (pin 2))
      (node (ref P1) (pin 4)))
    (net (code 4) (name "/GPIO2(SDA1)")
      (node (ref P1) (pin 3)))
    (net (code 5) (name +3V3)
      (node (ref P1) (pin 1))
      (node (ref P1) (pin 17)))
    (net (code 6) (name "/GPIO14(TXD0)")
      (node (ref P1) (pin 8)))
    (net (code 7) (name "/GPIO15(RXD0)")
      (node (ref P1) (pin 10)))
    (net (code 8) (name "/GPIO21(SPI1_SCK)")
      (node (ref P1) (pin 40)))
    (net (code 9) (name /GPIO5)
      (node (ref P1) (pin 29)))
    (net (code 10) (name "/GPIO20(SPI1_MOSI)")
      (node (ref P1) (pin 38)))
    (net (code 11) (name /ID_SC)
      (node (ref P1) (pin 28)))
    (net (code 12) (name "/GPIO24(GEN5)")
      (node (ref P1) (pin 18)))
    (net (code 13) (name /GPIO26)
      (node (ref P1) (pin 37)))
    (net (code 14) (name /ID_SD)
      (node (ref P1) (pin 27)))
    (net (code 15) (name /GPIO16)
      (node (ref P1) (pin 36)))
    (net (code 16) (name "/GPIO7(SPI1_CE_N)")
      (node (ref P1) (pin 26)))
    (net (code 17) (name "/GPIO23(GEN4)")
      (node (ref P1) (pin 16)))
    (net (code 18) (name "/GPIO19(SPI1_MISO)")
      (node (ref P1) (pin 35)))
    (net (code 19) (name "/GPIO8(SPI0_CE_N)")
      (node (ref P1) (pin 24)))
    (net (code 20) (name "/GPIO13(PWM1)")
      (node (ref P1) (pin 33)))
    (net (code 21) (name "/GPIO11(SPI0_SCK)")
      (node (ref P1) (pin 23)))
    (net (code 22) (name "/GPIO12(PWM0)")
      (node (ref P1) (pin 32)))
    (net (code 23) (name "/GPIO25(GEN6)")
      (node (ref P1) (pin 22)))
    (net (code 24) (name "/GPIO18(GEN1)(PWM0)")
      (node (ref P1) (pin 12)))
    (net (code 25) (name /GPIO6)
      (node (ref P1) (pin 31)))
    (net (code 26) (name "/GPIO9(SPI0_MISO)")
      (node (ref P1) (pin 21)))
    (net (code 27) (name GND)
      (node (ref P1) (pin 9))
      (node (ref P1) (pin 6))
      (node (ref P1) (pin 20))
      (node (ref P1) (pin 25))
      (node (ref P1) (pin 39))
      (node (ref P1) (pin 34))
      (node (ref P1) (pin 14))
      (node (ref P1) (pin 30)))
    (net (code 28) (name "/GPIO10(SPI0_MOSI)")
      (node (ref P1) (pin 19)))
    (net (code 29) (name "/GPIO22(GEN3)")
      (node (ref P1) (pin 15)))
    (net (code 30) (name "/GPIO27(GEN2)")
      (node (ref P1) (pin 13)))
    (net (code 31) (name "/GPIO17(GEN0)")
      (node (ref P1) (pin 11)))))