Metadata-Version: 1.1
Name: quisk
Version: 4.1.52
Summary: QUISK is a Software Defined Radio (SDR) transceiver that can control various radio hardware.
Home-page: http://james.ahlstrom.name/quisk/
Author: James C. Ahlstrom
Author-email: jahlstr@gmail.com
License: UNKNOWN
Description: QUISK is a Software Defined Radio (SDR) transceiver.  
        You supply radio hardware that converts signals at the antenna to complex (I/Q) data at an
        intermediate frequency (IF). Data can come from a sound card, Ethernet or USB. Quisk then filters and
        demodulates the data and sends the audio to your speakers or headphones. For transmit, Quisk takes
        the microphone signal, converts it to I/Q data and sends it to the hardware.
        
        Quisk can be used with SoftRock, Hermes Lite 2, HiQSDR, Odyssey and many radios that use the Hermes protocol.
        Quisk can connect to digital programs like Fldigi and WSJT-X. Quisk can be connected to other software like
        N1MM+ and software that uses Hamlib.
        
Platform: UNKNOWN
Classifier: Development Status :: 6 - Mature
Classifier: Environment :: X11 Applications
Classifier: Environment :: Win32 (MS Windows)
Classifier: Intended Audience :: End Users/Desktop
Classifier: License :: OSI Approved :: GNU General Public License (GPL)
Classifier: Natural Language :: English
Classifier: Operating System :: POSIX :: Linux
Classifier: Operating System :: Microsoft :: Windows
Classifier: Programming Language :: Python :: 2.7
Classifier: Programming Language :: Python :: 3
Classifier: Programming Language :: C
Classifier: Topic :: Communications :: Ham Radio
Provides: quisk
